######################################################################
## 
## $Id: sample-etc_ddclient.conf 8 2006-06-14 19:51:39Z wimpunk $
##
## Define default global variables with lines like:
## 	var=value [, var=value]*
## These values will be used for each following host unless overridden
## with a local variable definition.
##
## Define local variables for one or more hosts with:
## 	var=value [, var=value]* host.and.domain[,host2.and.domain...]
##
## Lines can be continued on the following line by ending the line
## with a \
##
##
## Warning: not all supported routers or dynamic DNS services 
##          are mentioned here.
##
######################################################################
daemon=300				# check every 300 seconds
syslog=yes				# log update msgs to syslog
mail=root				# mail all msgs to root
mail-failure=root			# mail failed update msgs to root
pid=/var/run/ddclient.pid		# record PID in file.
ssl=yes					# use ssl-support.  Works with
					# ssl-library
#
#use=watchguard-soho,        fw=192.168.111.1:80	# via Watchguard's SOHO FW
#use=netopia-r910,           fw=192.168.111.1:80	# via Netopia R910 FW
#use=smc-barricade,          fw=192.168.123.254:80	# via SMC's Barricade FW
#use=netgear-rt3xx,          fw=192.168.0.1:80		# via Netgear's internet FW
#use=linksys,                fw=192.168.1.1:80		# via Linksys's internet FW
#use=maxgate-ugate3x00,      fw=192.168.0.1:80		# via MaxGate's UGATE-3x00  FW
#use=elsa-lancom-dsl10,      fw=10.0.0.254:80		# via ELSA LanCom DSL/10 DSL Router
#use=elsa-lancom-dsl10-ch01, fw=10.0.0.254:80		# via ELSA LanCom DSL/10 DSL Router
#use=elsa-lancom-dsl10-ch02, fw=10.0.0.254:80		# via ELSA LanCom DSL/10 DSL Router
#use=alcatel-stp,            fw=10.0.0.138:80           # via Alcatel Speed Touch Pro
#use=xsense-aero,            fw=192.168.1.1:80          # via Xsense Aero Router
#use=allnet-1298,            fw=192.168.1.1:80          # via AllNet 1298 DSL Router
#use=3com-oc-remote812,	     fw=192.168.0.254:80	# via 3com OfficeConnect Remote 812
#use=e-tech,                 fw=192.168.1.1:80          # via E-tech Router
#use=cayman-3220h,           fw=192.168.0.1:1080        # via Cayman 3220-H DSL Router
#
#fw-login=admin,             fw-password=XXXXXX		# FW login and password
#
## To obtain an IP address from FW status page (using fw-login, fw-password)
#use=fw, fw=192.168.1.254/status.htm, fw-skip='IP Address' # found after IP Address
#
## To obtain an IP address from Web status page (using the proxy if defined)
#use=web, web=checkip.dyndns.org/, web-skip='IP Address' # found after IP Address
#
#use=ip,                     ip=127.0.0.1	# via static IP's
#use=if,                     if=eth0		# via interfaces
#use=web					# via web
#
#protocol=dyndns2				# default protocol
#proxy=fasthttp.sympatico.ca:80			# default proxy
#server=members.dyndns.org			# default server
#server=members.dyndns.org:8245			# default server (bypassing proxies)

login=your-login				# default login
password=test					# default password
#mx=mx.for.your.host				# default MX
#backupmx=yes|no				# host is primary MX?
#wildcard=yes|no				# add wildcard CNAME?


##
## (supports variables: wildcard,mx,backupmx)
##
 server=www.replacewithddnsserviceurl.com,		\
protocol=dyndns2			\
your-dynamic-host.dyndns.org




